
                                DRC - single_net
                                ----------------

                       09:31 AM Monday, February 22, 2021
        Job Name: E:\Compulab VX.2\FT-POE2-rev1.1\PCB\FT-POE2-rev1.1.pcb


    ---------
    PROXIMITY
    ---------
    
    Use DRC Window                   : NO


    Disable Same Cell Pad-Pad Checks : YES


    Enable Same Net Pad-Pad Checks   : NO

    
    Layers Specifed To Check         : Layer 1
                                       Layer 2
                                       Layer 3
                                       Layer 4
                                       Layer 5
                                       Layer 6




    Net Class Clearances And Rules
    ------------------------------

        Components Layer 1 TO Components Layer 1
            No Hazards.

        Traces Layer 1 TO Traces Layer 1
            No Hazards.

        Traces Layer 1 TO Differential Pair Traces Layer 1
            No Hazards.

        Traces Layer 1 TO Mounting Hole Pads Layer 1
            No Hazards.

        Traces Layer 1 TO Part Pads SMD Layer 1
            No Hazards.

        Traces Layer 1 TO Part Pads Thru Layer 1
            No Hazards.

        Traces Layer 1 TO Part Holes Layer 1
            No Hazards.

        Traces Layer 1 TO Via Pads Layer 1
            No Hazards.

        Traces Layer 1 TO Via Holes Layer 1
            No Hazards.

        Differential Pair Traces Layer 1 TO Differential Pair Traces Layer 1
            No Hazards.

        Differential Pair Traces Layer 1 TO Mounting Hole Pads Layer 1
            No Hazards.

        Differential Pair Traces Layer 1 TO Part Pads SMD Layer 1
            No Hazards.

        Differential Pair Traces Layer 1 TO Part Pads Thru Layer 1
            No Hazards.

        Differential Pair Traces Layer 1 TO Part Holes Layer 1
            No Hazards.

        Differential Pair Traces Layer 1 TO Via Pads Layer 1
            No Hazards.

        Differential Pair Traces Layer 1 TO Via Holes Layer 1
            No Hazards.

        Mounting Hole Pads Layer 1 TO Mounting Hole Pads Layer 1
            No Hazards.

        Mounting Hole Pads Layer 1 TO Part Pads SMD Layer 1
            No Hazards.

        Mounting Hole Pads Layer 1 TO Part Pads Thru Layer 1
            No Hazards.

        Mounting Hole Pads Layer 1 TO Part Holes Layer 1
            No Hazards.

        Mounting Hole Pads Layer 1 TO Via Pads Layer 1
            No Hazards.

        Mounting Hole Pads Layer 1 TO Via Holes Layer 1
            No Hazards.

        Part Pads SMD Layer 1 TO Part Pads SMD Layer 1
            No Hazards.

        Part Pads SMD Layer 1 TO Part Pads Thru Layer 1
            No Hazards.

        Part Pads SMD Layer 1 TO Part Holes Layer 1
            No Hazards.

        Part Pads SMD Layer 1 TO Via Pads Layer 1
            No Hazards.

        Part Pads SMD Layer 1 TO Via Holes Layer 1
            No Hazards.

        Part Pads Thru Layer 1 TO Part Pads Thru Layer 1
            No Hazards.

        Part Pads Thru Layer 1 TO Part Holes Layer 1
            No Hazards.

        Part Pads Thru Layer 1 TO Via Pads Layer 1
            No Hazards.

        Part Pads Thru Layer 1 TO Via Holes Layer 1
            No Hazards.

        Part Holes Layer 1 TO Via Pads Layer 1
            No Hazards.

        Part Holes Layer 1 TO Via Holes Layer 1
            No Hazards.

        Via Pads Layer 1 TO Via Pads Layer 1
            No Hazards.

        Via Pads Layer 1 TO Via Holes Layer 1
            No Hazards.

        Via Holes Layer 1 TO Via Holes Layer 1
            No Hazards.

        Traces Layer 1 TO Fiducial Pads Top
            No Hazards.

        Differential Pair Traces Layer 1 TO Fiducial Pads Top
            No Hazards.

        Fiducial Pads Top TO Fiducial Pads Top
            No Hazards.

        Fiducial Pads Top TO Mounting Hole Pads Layer 1
            No Hazards.

        Fiducial Pads Top TO Part Pads SMD Layer 1
            No Hazards.

        Fiducial Pads Top TO Part Pads Thru Layer 1
            No Hazards.

        Fiducial Pads Top TO Part Holes Layer 1
            No Hazards.

        Fiducial Pads Top TO Via Pads Layer 1
            No Hazards.

        Fiducial Pads Top TO Via Holes Layer 1
            No Hazards.

        User Text Route Layer 2 TO Mounting Hole Pads Layer 2
            No Hazards.

        User Text Route Layer 2 TO Part Pads Thru Layer 2
            No Hazards.

        User Text Route Layer 2 TO Part Holes Layer 2
            No Hazards.

        User Text Route Layer 2 TO Via Pads Layer 2
            No Hazards.

        User Text Route Layer 2 TO Via Holes Layer 2
            No Hazards.

        Mounting Hole Pads Layer 2 TO Mounting Hole Pads Layer 2
            No Hazards.

        Mounting Hole Pads Layer 2 TO Part Pads Thru Layer 2
            No Hazards.

        Mounting Hole Pads Layer 2 TO Part Holes Layer 2
            No Hazards.

        Mounting Hole Pads Layer 2 TO Via Pads Layer 2
            No Hazards.

        Mounting Hole Pads Layer 2 TO Via Holes Layer 2
            No Hazards.

        Part Pads Thru Layer 2 TO Part Pads Thru Layer 2
            No Hazards.

        Part Pads Thru Layer 2 TO Part Holes Layer 2
            No Hazards.

        Part Pads Thru Layer 2 TO Via Pads Layer 2
            No Hazards.

        Part Pads Thru Layer 2 TO Via Holes Layer 2
            No Hazards.

        Part Holes Layer 2 TO Via Pads Layer 2
            No Hazards.

        Part Holes Layer 2 TO Via Holes Layer 2
            No Hazards.

        Via Pads Layer 2 TO Via Pads Layer 2
            No Hazards.

        Via Pads Layer 2 TO Via Holes Layer 2
            No Hazards.

        Via Holes Layer 2 TO Via Holes Layer 2
            No Hazards.

        Traces Layer 3 TO Traces Layer 3
            No Hazards.

        Traces Layer 3 TO Differential Pair Traces Layer 3
            No Hazards.

        Traces Layer 3 TO Mounting Hole Pads Layer 3
            No Hazards.

        Traces Layer 3 TO Part Pads Thru Layer 3
            No Hazards.

        Traces Layer 3 TO Part Holes Layer 3
            No Hazards.

        Traces Layer 3 TO Via Pads Layer 3
            No Hazards.

        Traces Layer 3 TO Via Holes Layer 3
            No Hazards.

        Traces Layer 3 TO User Text Route Layer 3
            No Hazards.

        User Text Route Layer 3 TO Differential Pair Traces Layer 3
            No Hazards.

        User Text Route Layer 3 TO Mounting Hole Pads Layer 3
            No Hazards.

        User Text Route Layer 3 TO Part Pads Thru Layer 3
            No Hazards.

        User Text Route Layer 3 TO Part Holes Layer 3
            No Hazards.

        User Text Route Layer 3 TO Via Pads Layer 3
            No Hazards.

        User Text Route Layer 3 TO Via Holes Layer 3
            No Hazards.

        Differential Pair Traces Layer 3 TO Differential Pair Traces Layer 3
            No Hazards.

        Differential Pair Traces Layer 3 TO Mounting Hole Pads Layer 3
            No Hazards.

        Differential Pair Traces Layer 3 TO Part Pads Thru Layer 3
            No Hazards.

        Differential Pair Traces Layer 3 TO Part Holes Layer 3
            No Hazards.

        Differential Pair Traces Layer 3 TO Via Pads Layer 3
            No Hazards.

        Differential Pair Traces Layer 3 TO Via Holes Layer 3
            No Hazards.

        Mounting Hole Pads Layer 3 TO Mounting Hole Pads Layer 3
            No Hazards.

        Mounting Hole Pads Layer 3 TO Part Pads Thru Layer 3
            No Hazards.

        Mounting Hole Pads Layer 3 TO Part Holes Layer 3
            No Hazards.

        Mounting Hole Pads Layer 3 TO Via Pads Layer 3
            No Hazards.

        Mounting Hole Pads Layer 3 TO Via Holes Layer 3
            No Hazards.

        Part Pads Thru Layer 3 TO Part Pads Thru Layer 3
            No Hazards.

        Part Pads Thru Layer 3 TO Part Holes Layer 3
            No Hazards.

        Part Pads Thru Layer 3 TO Via Pads Layer 3
            No Hazards.

        Part Pads Thru Layer 3 TO Via Holes Layer 3
            No Hazards.

        Part Holes Layer 3 TO Via Pads Layer 3
            No Hazards.

        Part Holes Layer 3 TO Via Holes Layer 3
            No Hazards.

        Via Pads Layer 3 TO Via Pads Layer 3
            No Hazards.

        Via Pads Layer 3 TO Via Holes Layer 3
            No Hazards.

        Via Holes Layer 3 TO Via Holes Layer 3
            No Hazards.

        Traces Layer 4 TO Traces Layer 4
            No Hazards.

        Traces Layer 4 TO Differential Pair Traces Layer 4
            No Hazards.

        Traces Layer 4 TO Mounting Hole Pads Layer 4
            No Hazards.

        Traces Layer 4 TO Part Pads Thru Layer 4
            No Hazards.

        Traces Layer 4 TO Part Holes Layer 4
            No Hazards.

        Traces Layer 4 TO Via Pads Layer 4
            No Hazards.

        Traces Layer 4 TO Via Holes Layer 4
            No Hazards.

        Traces Layer 4 TO User Text Route Layer 4
            No Hazards.

        User Text Route Layer 4 TO Differential Pair Traces Layer 4
            No Hazards.

        User Text Route Layer 4 TO Mounting Hole Pads Layer 4
            No Hazards.

        User Text Route Layer 4 TO Part Pads Thru Layer 4
            No Hazards.

        User Text Route Layer 4 TO Part Holes Layer 4
            No Hazards.

        User Text Route Layer 4 TO Via Pads Layer 4
            No Hazards.

        User Text Route Layer 4 TO Via Holes Layer 4
            No Hazards.

        Differential Pair Traces Layer 4 TO Differential Pair Traces Layer 4
            No Hazards.

        Differential Pair Traces Layer 4 TO Mounting Hole Pads Layer 4
            No Hazards.

        Differential Pair Traces Layer 4 TO Part Pads Thru Layer 4
            No Hazards.

        Differential Pair Traces Layer 4 TO Part Holes Layer 4
            No Hazards.

        Differential Pair Traces Layer 4 TO Via Pads Layer 4
            No Hazards.

        Differential Pair Traces Layer 4 TO Via Holes Layer 4
            No Hazards.

        Mounting Hole Pads Layer 4 TO Mounting Hole Pads Layer 4
            No Hazards.

        Mounting Hole Pads Layer 4 TO Part Pads Thru Layer 4
            No Hazards.

        Mounting Hole Pads Layer 4 TO Part Holes Layer 4
            No Hazards.

        Mounting Hole Pads Layer 4 TO Via Pads Layer 4
            No Hazards.

        Mounting Hole Pads Layer 4 TO Via Holes Layer 4
            No Hazards.

        Part Pads Thru Layer 4 TO Part Pads Thru Layer 4
            No Hazards.

        Part Pads Thru Layer 4 TO Part Holes Layer 4
            No Hazards.

        Part Pads Thru Layer 4 TO Via Pads Layer 4
            No Hazards.

        Part Pads Thru Layer 4 TO Via Holes Layer 4
            No Hazards.

        Part Holes Layer 4 TO Via Pads Layer 4
            No Hazards.

        Part Holes Layer 4 TO Via Holes Layer 4
            No Hazards.

        Via Pads Layer 4 TO Via Pads Layer 4
            No Hazards.

        Via Pads Layer 4 TO Via Holes Layer 4
            No Hazards.

        Via Holes Layer 4 TO Via Holes Layer 4
            No Hazards.

        User Text Route Layer 5 TO Mounting Hole Pads Layer 5
            No Hazards.

        User Text Route Layer 5 TO Part Pads Thru Layer 5
            No Hazards.

        User Text Route Layer 5 TO Part Holes Layer 5
            No Hazards.

        User Text Route Layer 5 TO Via Pads Layer 5
            No Hazards.

        User Text Route Layer 5 TO Via Holes Layer 5
            No Hazards.

        Mounting Hole Pads Layer 5 TO Mounting Hole Pads Layer 5
            No Hazards.

        Mounting Hole Pads Layer 5 TO Part Pads Thru Layer 5
            No Hazards.

        Mounting Hole Pads Layer 5 TO Part Holes Layer 5
            No Hazards.

        Mounting Hole Pads Layer 5 TO Via Pads Layer 5
            No Hazards.

        Mounting Hole Pads Layer 5 TO Via Holes Layer 5
            No Hazards.

        Part Pads Thru Layer 5 TO Part Pads Thru Layer 5
            No Hazards.

        Part Pads Thru Layer 5 TO Part Holes Layer 5
            No Hazards.

        Part Pads Thru Layer 5 TO Via Pads Layer 5
            No Hazards.

        Part Pads Thru Layer 5 TO Via Holes Layer 5
            No Hazards.

        Part Holes Layer 5 TO Via Pads Layer 5
            No Hazards.

        Part Holes Layer 5 TO Via Holes Layer 5
            No Hazards.

        Via Pads Layer 5 TO Via Pads Layer 5
            No Hazards.

        Via Pads Layer 5 TO Via Holes Layer 5
            No Hazards.

        Via Holes Layer 5 TO Via Holes Layer 5
            No Hazards.

    >>  Components Layer 6 TO Components Layer 6
            Hazards Found : 3

        Traces Layer 6 TO Traces Layer 6
            No Hazards.

        Traces Layer 6 TO Differential Pair Traces Layer 6
            No Hazards.

        Traces Layer 6 TO Mounting Hole Pads Layer 6
            No Hazards.

        Traces Layer 6 TO Part Pads SMD Layer 6
            No Hazards.

        Traces Layer 6 TO Part Pads Thru Layer 6
            No Hazards.

        Traces Layer 6 TO Part Holes Layer 6
            No Hazards.

        Traces Layer 6 TO Via Pads Layer 6
            No Hazards.

        Traces Layer 6 TO Via Holes Layer 6
            No Hazards.

        Traces Layer 6 TO User Text Route Layer 6
            No Hazards.

        User Text Route Layer 6 TO Differential Pair Traces Layer 6
            No Hazards.

        User Text Route Layer 6 TO Mounting Hole Pads Layer 6
            No Hazards.

        User Text Route Layer 6 TO Part Pads SMD Layer 6
            No Hazards.

        User Text Route Layer 6 TO Part Pads Thru Layer 6
            No Hazards.

        User Text Route Layer 6 TO Part Holes Layer 6
            No Hazards.

        User Text Route Layer 6 TO Via Pads Layer 6
            No Hazards.

        User Text Route Layer 6 TO Via Holes Layer 6
            No Hazards.

        Differential Pair Traces Layer 6 TO Differential Pair Traces Layer 6
            No Hazards.

        Differential Pair Traces Layer 6 TO Mounting Hole Pads Layer 6
            No Hazards.

        Differential Pair Traces Layer 6 TO Part Pads SMD Layer 6
            No Hazards.

        Differential Pair Traces Layer 6 TO Part Pads Thru Layer 6
            No Hazards.

        Differential Pair Traces Layer 6 TO Part Holes Layer 6
            No Hazards.

        Differential Pair Traces Layer 6 TO Via Pads Layer 6
            No Hazards.

        Differential Pair Traces Layer 6 TO Via Holes Layer 6
            No Hazards.

        Mounting Hole Pads Layer 6 TO Mounting Hole Pads Layer 6
            No Hazards.

        Mounting Hole Pads Layer 6 TO Part Pads SMD Layer 6
            No Hazards.

        Mounting Hole Pads Layer 6 TO Part Pads Thru Layer 6
            No Hazards.

        Mounting Hole Pads Layer 6 TO Part Holes Layer 6
            No Hazards.

        Mounting Hole Pads Layer 6 TO Via Pads Layer 6
            No Hazards.

        Mounting Hole Pads Layer 6 TO Via Holes Layer 6
            No Hazards.

        Part Pads SMD Layer 6 TO Part Pads SMD Layer 6
            No Hazards.

        Part Pads SMD Layer 6 TO Part Pads Thru Layer 6
            No Hazards.

        Part Pads SMD Layer 6 TO Part Holes Layer 6
            No Hazards.

        Part Pads SMD Layer 6 TO Via Pads Layer 6
            No Hazards.

        Part Pads SMD Layer 6 TO Via Holes Layer 6
            No Hazards.

        Part Pads Thru Layer 6 TO Part Pads Thru Layer 6
            No Hazards.

        Part Pads Thru Layer 6 TO Part Holes Layer 6
            No Hazards.

        Part Pads Thru Layer 6 TO Via Pads Layer 6
            No Hazards.

        Part Pads Thru Layer 6 TO Via Holes Layer 6
            No Hazards.

        Part Holes Layer 6 TO Via Pads Layer 6
            No Hazards.

        Part Holes Layer 6 TO Via Holes Layer 6
            No Hazards.

        Via Pads Layer 6 TO Via Pads Layer 6
            No Hazards.

        Via Pads Layer 6 TO Via Holes Layer 6
            No Hazards.

        Via Holes Layer 6 TO Via Holes Layer 6
            No Hazards.

        Traces Layer 6 TO Fiducial Pads Bottom
            No Hazards.

        User Text Route Layer 6 TO Fiducial Pads Bottom
            No Hazards.

        Differential Pair Traces Layer 6 TO Fiducial Pads Bottom
            No Hazards.

        Fiducial Pads Bottom TO Fiducial Pads Bottom
            No Hazards.

        Fiducial Pads Bottom TO Mounting Hole Pads Layer 6
            No Hazards.

        Fiducial Pads Bottom TO Part Pads SMD Layer 6
            No Hazards.

        Fiducial Pads Bottom TO Part Pads Thru Layer 6
            No Hazards.

        Fiducial Pads Bottom TO Part Holes Layer 6
            No Hazards.

        Fiducial Pads Bottom TO Via Pads Layer 6
            No Hazards.

        Fiducial Pads Bottom TO Via Holes Layer 6
            No Hazards.


        Total Hazards Found : 3




    Planes Clearances And Rules
    ---------------------------

        Positive Planes Layer 1 TO Differential Pair Traces Layer 1
            No Hazards.

        Positive Planes Layer 1 TO Mounting Hole Pads Layer 1
            No Hazards.

        Positive Planes Layer 1 TO Mounting Holes Layer 1
            No Hazards.

        Positive Planes Layer 1 TO Part Pads SMD Layer 1
            No Hazards.

        Positive Planes Layer 1 TO Part Pads Thru Layer 1
            No Hazards.

        Positive Planes Layer 1 TO Part Holes Layer 1
            No Hazards.

        Positive Planes Layer 1 TO Positive Planes Layer 1
            No Hazards.

        Positive Planes Layer 1 TO Route Border
            No Hazards.

        Positive Planes Layer 1 TO Traces Layer 1
            No Hazards.

        Positive Planes Layer 1 TO Trace Obstructs Layer 1
            No Hazards.

        Positive Planes Layer 1 TO Plane Obstructs Layer 1
            No Hazards.

        Positive Planes Layer 1 TO Via Pads Layer 1
            No Hazards.

        Positive Planes Layer 1 TO Via Holes Layer 1
            No Hazards.

        Positive Planes Layer 1 TO Fiducial Pads Top
            No Hazards.

        Positive Planes Layer 2 TO Mounting Hole Pads Layer 2
            No Hazards.

        Positive Planes Layer 2 TO Mounting Holes Layer 2
            No Hazards.

        Positive Planes Layer 2 TO Part Pads Thru Layer 2
            No Hazards.

        Positive Planes Layer 2 TO Part Holes Layer 2
            No Hazards.

        Positive Planes Layer 2 TO Positive Planes Layer 2
            No Hazards.

        Positive Planes Layer 2 TO Route Border
            No Hazards.

        Positive Planes Layer 2 TO User Text Route Layer 2
            No Hazards.

        Positive Planes Layer 2 TO Trace Obstructs Layer 2
            No Hazards.

        Positive Planes Layer 2 TO Plane Obstructs Layer 2
            No Hazards.

        Positive Planes Layer 2 TO Via Pads Layer 2
            No Hazards.

        Positive Planes Layer 2 TO Via Holes Layer 2
            No Hazards.

        Positive Planes Layer 3 TO Differential Pair Traces Layer 3
            No Hazards.

        Positive Planes Layer 3 TO Mounting Hole Pads Layer 3
            No Hazards.

        Positive Planes Layer 3 TO Mounting Holes Layer 3
            No Hazards.

        Positive Planes Layer 3 TO Part Pads Thru Layer 3
            No Hazards.

        Positive Planes Layer 3 TO Part Holes Layer 3
            No Hazards.

        Positive Planes Layer 3 TO Positive Planes Layer 3
            No Hazards.

        Positive Planes Layer 3 TO Route Border
            No Hazards.

        Positive Planes Layer 3 TO Traces Layer 3
            No Hazards.

        Positive Planes Layer 3 TO User Text Route Layer 3
            No Hazards.

        Positive Planes Layer 3 TO Trace Obstructs Layer 3
            No Hazards.

        Positive Planes Layer 3 TO Plane Obstructs Layer 3
            No Hazards.

        Positive Planes Layer 3 TO Via Pads Layer 3
            No Hazards.

        Positive Planes Layer 3 TO Via Holes Layer 3
            No Hazards.

        Positive Planes Layer 4 TO Differential Pair Traces Layer 4
            No Hazards.

        Positive Planes Layer 4 TO Mounting Hole Pads Layer 4
            No Hazards.

        Positive Planes Layer 4 TO Mounting Holes Layer 4
            No Hazards.

        Positive Planes Layer 4 TO Part Pads Thru Layer 4
            No Hazards.

        Positive Planes Layer 4 TO Part Holes Layer 4
            No Hazards.

        Positive Planes Layer 4 TO Positive Planes Layer 4
            No Hazards.

        Positive Planes Layer 4 TO Route Border
            No Hazards.

        Positive Planes Layer 4 TO Traces Layer 4
            No Hazards.

        Positive Planes Layer 4 TO User Text Route Layer 4
            No Hazards.

        Positive Planes Layer 4 TO Trace Obstructs Layer 4
            No Hazards.

        Positive Planes Layer 4 TO Plane Obstructs Layer 4
            No Hazards.

        Positive Planes Layer 4 TO Via Pads Layer 4
            No Hazards.

        Positive Planes Layer 4 TO Via Holes Layer 4
            No Hazards.

        Positive Planes Layer 5 TO Mounting Hole Pads Layer 5
            No Hazards.

        Positive Planes Layer 5 TO Mounting Holes Layer 5
            No Hazards.

        Positive Planes Layer 5 TO Part Pads Thru Layer 5
            No Hazards.

        Positive Planes Layer 5 TO Part Holes Layer 5
            No Hazards.

        Positive Planes Layer 5 TO Positive Planes Layer 5
            No Hazards.

        Positive Planes Layer 5 TO Route Border
            No Hazards.

        Positive Planes Layer 5 TO User Text Route Layer 5
            No Hazards.

        Positive Planes Layer 5 TO Trace Obstructs Layer 5
            No Hazards.

        Positive Planes Layer 5 TO Plane Obstructs Layer 5
            No Hazards.

        Positive Planes Layer 5 TO Via Pads Layer 5
            No Hazards.

        Positive Planes Layer 5 TO Via Holes Layer 5
            No Hazards.

        Positive Planes Layer 6 TO Differential Pair Traces Layer 6
            No Hazards.

        Positive Planes Layer 6 TO Mounting Hole Pads Layer 6
            No Hazards.

        Positive Planes Layer 6 TO Mounting Holes Layer 6
            No Hazards.

        Positive Planes Layer 6 TO Part Pads SMD Layer 6
            No Hazards.

        Positive Planes Layer 6 TO Part Pads Thru Layer 6
            No Hazards.

        Positive Planes Layer 6 TO Part Holes Layer 6
            No Hazards.

        Positive Planes Layer 6 TO Positive Planes Layer 6
            No Hazards.

        Positive Planes Layer 6 TO Route Border
            No Hazards.

        Positive Planes Layer 6 TO Traces Layer 6
            No Hazards.

        Positive Planes Layer 6 TO User Text Route Layer 6
            No Hazards.

        Positive Planes Layer 6 TO Trace Obstructs Layer 6
            No Hazards.

        Positive Planes Layer 6 TO Plane Obstructs Layer 6
            No Hazards.

        Positive Planes Layer 6 TO Via Pads Layer 6
            No Hazards.

        Positive Planes Layer 6 TO Via Holes Layer 6
            No Hazards.

        Positive Planes Layer 6 TO Fiducial Pads Bottom
            No Hazards.


        Total Hazards Found : 0




    Test Probe Clearances And Rules
    ------------------------------

    Test Probe Checks Not Selected.




    Bond Wire Clearances And Rules
    ------------------------------

    Bond Wire Checks Not Selected.




    Non-Net Class Element To Element Clearances And Rules
    -----------------------------------------------------

    Non-Net Class Element To Element Checks Not Selected.



    Total Proximity Hazards Found : 3




    ----------------------------
    CONNECTIVITY & SPECIAL RULES
    ----------------------------


    Check For Unplaced Parts                      : YES
        No Hazards.


    Check For Missing Parts                       : YES
        No Hazards.


    Check EP Component Hazards                    : YES
        No Hazards.


    Check Test Probe Hazards                      : NO


    Check Bond Wire Hazards                       : NO


    Check Trace Hangers                           : YES
        No Hazards.


    Check Trace Loops                             : NO


    Check Trace Widths                            : NO


    Check Single Point Nets                       : YES
        No Hazards.


    Check NonPlane Unrouted/Partially Routed Nets : YES
        No Hazards.


    Check Plane Unrouted/Partial Routed Nets      : YES
        No Hazards.


    Check Routed Plane Pins                       : YES
        No Hazards.


    Check Plane Islands                           : NO


    Check Dangling Vias/Jumpers                   : YES
        No Hazards.


    Check Unrouted Pins                           : NO


    Check Routed Non-Plated Pins                  : YES
        No Hazards.


    Check Minimum Annular Ring                    : NO


    Check For Vias Under SMD Pads                 : YES
        No Hazards.


    Check For Vias Under Top Place Outlines       : NO


    Check For Vias Under Bottom Place Outlines    : NO


    Check For Missing Conductive Pads             : All Pads / All Layers
        No Hazards.


    Check For Missing Part Soldermask Pads        : YES
        No Hazards.


    Check For Missing Via Soldermask Pads         : NO


    Check For Missing Part Cover Layer Pads       : NO


    Check For Missing Via Cover Layer Pads        : NO


    Check For Missing Solderpaste Pads            : YES
        Hazards Found : 3



    Total Connectivity/SpecialRules Hazards Found : 3



    ====================================================================



    Total DRC Hazards Found : 6



                         09:31 AM Monday, February 22, 2021